Question :

# Assignment -4

|  |  |
| --- | --- |
| Assignment Date | 06 November 2022 |
| Student Name | Hema Priyyan S |
| Student Register Number | 312419104051 |
| Maximum Marks | 2 Marks |

Write a code and connections in wokwi for the ultrasonic sensor. Whenever the distance is less than 100cms send an “Alert” to IBM cloud and display in the device recent events.

# Code:

#include <WiFi.h> #include

<PubSubClient.h>

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength);

//-------credentials of IBM Accounts------

#define ORG "kotoq5"//IBM ORGANITION ID

#define DEVICE\_TYPE "ESP32"//Device type mentioned in ibm watson IOT Platform #define DEVICE\_ID "12345"//Device ID mentioned in ibm watson IOT Platform #define TOKEN "12345678" //Token

String data3;

char server[] = ORG ".messaging.internetofthings.ibmcloud.com"; char publishTopic[] = "iot-2/evt/Data/fmt/json";

char subscribetopic[] = "iot-2/cmd/test/fmt/String"; char authMethod[] = "use-token-auth";

char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;

WiFiClient wifiClient;

PubSubClient client(server, 1883, callback ,wifiClient); const int trigPin = 5;

const int echoPin = 18; #define SOUND\_SPEED

0.034 long duration; float

distance; void setup() { **Serial**.begin(115200);

pinMode(trigPin, OUTPUT); pinMode(echoPin, INPUT); wificonnect(); mqttconnect();

}

void loop()

{

digitalWrite(trigPin, LOW); delayMicroseconds(2); digitalWrite(trigPin, HIGH); delayMicroseconds(10); digitalWrite(trigPin, LOW); duration = pulseIn(echoPin, HIGH); distance = duration \* SOUND\_SPEED/2;

**Serial**.print("Distance (cm): "); **Serial**.println(distance); if(distance<100)

{

**Serial**.println("ALERT!!"); delay(1000);

PublishData(distance)

; delay(1000);

if (!client.loop()) { mqttconnect();

}

}

delay(1000);

}

void PublishData(float dist) { mqttconnect();

String payload = "{\"Distance\":"; payload += dist;

payload += ",\"ALERT!!\":""\"Distance less than 100cms\""; payload += "}";

**Serial**.print("Sending payload: ");

**Serial**.println(payload);

if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish ok");

} else {

**Serial**.println("Publish failed");

}

}

void mqttconnect() {

if (!client.connected()) { **Serial**.print("Reconnecting client to "); **Serial**.println(server);

while (!!!client.connect(clientId, authMethod, token)) {

**Serial**.print(".")

; delay(500);

}

initManagedDevice();

**Serial**.println();

}

}

void wificonnect()

{

**Serial**.println(); **Serial**.print("Connecting to "); WiFi.begin("Wokwi-GUEST", "", 6); while (WiFi.status() != WL\_CONNECTED) { delay(500);

**Serial**.print(".");

}

**Serial**.println(""); **Serial**.println("WiFi connected"); **Serial**.println("IP address: "); **Serial**.println(WiFi.localIP());

}

void initManagedDevice() {

if (client.subscribe(subscribetopic)) { **Serial**.println((subscribetopic)); **Serial**.println("subscribe to cmd OK");

} else {

**Serial**.println("subscribe to cmd FAILED");

}

}

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength)

{

**Serial**.print("callback invoked for topic: ");

**Serial**.println(subscribetopic);

for (int i = 0; i < payloadLength; i++) {

//Serial.print((char)payload[i])

; data3 += (char)payload[i];

}

**Serial**.println("data: "+ data3); data3="";

}

# Diagram.json:

{

"version": 1,

"author": "Smart ", "editor": "wokwi",

"parts": [

{ "type": "wokwi-esp32-devkit-v1", "id": "esp", "top": 10.67, "left": -133.33, "attrs": {} },

{ "type": "wokwi-hc-sr04", "id": "ultrasonic1", "top": -31.37, "left": 45.17, "attrs": {} }

],

"connections": [

[ "esp:TX0", "$serialMonitor:RX", "", [] ],

[ "esp:RX0", "$serialMonitor:TX", "", [] ], [

"ultrasonic1:VCC", "esp:VIN",

"red",

[ "v93.91", "h-100.45", "v-168", "h-186", "v181.33", "h-6.67" ]

],

[ "ultrasonic1:TRIG", "esp:D5", "green", [ "v42.57", "h-158.34" ] ],


[ "ultrasonic1:ECHO", "esp:D18", "green", [ "v116.57", "h-80.23", "v0" ] ],

[ "ultrasonic1:GND", "esp:GND.1", "black", [ "v141.91", "h-133.45", "v-38.67" ] ]

]


}

Crcuit Diagram:



# Output:

Wokwi output:



# IBM cloud output:

